Building configuration...

Current configuration : 1484 bytes

!

! Last configuration change at 01:24:47 UTC Mon Jan 2 2006

version 15.3

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

!

hostname NAT\_DHCP

!

boot-start-marker

boot-end-marker

!

!

!

no aaa new-model

dot11 syslog

!

!

ip dhcp excluded-address 192.168.0.1

!

ip dhcp pool ADRESY

network 192.168.0.0 255.255.255.0

dns-server 158.193.152.2

default-router 192.168.0.1

!

ip dhcp pool adresy

!

!

!

!

no ip domain lookup

ip cef

no ipv6 cef

!

multilink bundle-name authenticated

!

!

!

!

!

license udi pid CISCO1841 sn FCZ094912XT

username admin privilege 15 password 0 admin

!

redundancy

!

!

controller DSL 0/1/0

!

!

!

!

!

!

!

!

!

!

interface FastEthernet0/0

ip address dhcp

ip nat outside

ip virtual-reassembly in

duplex auto

speed auto

!

interface FastEthernet0/1

ip address 192.168.0.1 255.255.255.0

ip nat inside

ip virtual-reassembly in

duplex auto

speed auto

!

interface Serial0/0/0

no ip address

shutdown

clock rate 2000000

!

interface Serial0/0/1

no ip address

shutdown

clock rate 2000000

!

ip forward-protocol nd

no ip http server

no ip http secure-server

!

!

ip nat inside source list 100 interface FastEthernet0/0 overload

!

!

!

access-list 100 permit ip 192.168.0.0 0.0.0.255 any

!

control-plane

!

!

!

line con 0

line aux 0

line vty 0 4

logging synchronous

login local

transport input all

line vty 5 15

logging synchronous

login local

transport input all

!

scheduler allocate 20000 1000

!

end